Sensor Calibration:

Air: Analog = 230, Voltage = 2.99

Water: Analog = 102, Voltage = 1.32